**§1632. Enclosure of swimming pool required**

A fence shall be erected and maintained around every swimming pool, except that portable above-ground swimming pools with sidewalls of at least 24 inches in height are exempted. A dwelling house or accessory building may be used as part of this enclosure. All gates or doors opening through this enclosure shall be capable of being securely fastened at all times when not in actual use. [PL 1983, c. 436 (NEW).]

SECTION HISTORY

PL 1983, c. 436 (NEW).

The State of Maine claims a copyright in its codified statutes. If you intend to republish this material, we require that you include the following disclaimer in your publication:

*All copyrights and other rights to statutory text are reserved by the State of Maine. The text included in this publication reflects changes made through the Second Regular Session of the 131st Maine Legislature and is current through January 1, 2025
. The text is subject to change without notice. It is a version that has not been officially certified by the Secretary of State. Refer to the Maine Revised Statutes Annotated and supplements for certified text.*

The Office of the Revisor of Statutes also requests that you send us one copy of any statutory publication you may produce. Our goal is not to restrict publishing activity, but to keep track of who is publishing what, to identify any needless duplication and to preserve the State's copyright rights.

PLEASE NOTE: The Revisor's Office cannot perform research for or provide legal advice or interpretation of Maine law to the public. If you need legal assistance, please contact a qualified attorney.